

**USER MANUAL**

STAND FAN WITH REMOTE CONTROL

Model：RHPF16



READ AND SAVE THESE SAFETY INSTRUCTIONS BEFORE USING THIS APPLIANCE

**IMPORTANT SAFETY INSTRUCTIONS**

**WARNING:** When using electrical appliance, basic safety precautions should always be followed to reduce the risk of fire, electrical shock and personal injury.

Use this fan only as described in this manual. Other use not recommended may cause fire, electric shock or injury to persons.

This product is intended for household use ONLY and not for commercial, industrial or outdoor use.

To protect against electric shock: do not place fan on windowsills, immerse unit, plug or cord in water or spray with liquids.

To reduce the risk of shock, this plug is intended to fit the outlet. If the plug does not fit fully in the outlet, reverse the plug. If it still does not fit, contact a qualified electrician. DO NOT attempt to defeat this safety feature.

**To reduce the risk of fire or electric shock, do not use this fan with any solid-state speed control device.**

This appliance is not intended for use by person (including children) with reduced physical, sensory or mental capabilities, or lack of experience and knowledge, unless they have been given supervision or instruction concerning use of the appliance by a person responsible for their safety.

Children should be supervised to ensure that they do not play with the appliance.

Turn the fan OFF and unplug the fan from the outlet when not in use, when moving the fan from one location to another and before cleaning.

To disconnect the fan, first turn the unit OFF, grip the plug and pull it from the wall outlet. Never pull the plug by the cord.

Do not operate the fan in the presence of explosive and/or flammable fumes.

Do not place the fan or any parts near an open flame, cooking or other heating appliance.

Do not operate fan with a damaged cord or plug, or if the product malfunctions, or dropped and damaged in any manner.

Avoid contact with moving fan parts.

The use of attachments not recommended by the manufacturer may be hazardous.

Place the fan on a dry level surface.

Do not hang or mount fan on a wall or ceiling.

Do not operate if the fan housing is damaged.


A loose fit between the AC outlet (receptacle) and plug may cause overheating and a distortion of the plug. Contact a qualified electrician to replace loose or worn outlet.

Only use on a power supply that matches that shown on the unit’s rating label.

If the supply cord is damaged, it must be replaced by the manufacturer, its service agent or similarly qualified persons in order to avoid hazard.

**MAIN TECHNICAL DATA**

|  |  |
| --- | --- |
| **techniCAL cHaractEristiCs** | |
| Model No.: | PHPF16 |
| Rated Voltage: | 220V – 240v~ |
| Rated Frequency: | 50Hz |
| Power Input: | 50W |
| Protection Class | II |
| Blade Size: | 400 mm |

**Parts Identification / assembly**

**1) Parts Identification**

|  |  |  |
| --- | --- | --- |
| iNDEX | | pART NAME |
| [1] | **:** | Fan grill |
| [2] | **:** | Display panel |
| [3] | **:** | Fan body |
| [4] | **:** | Base |
| [5] | **:** | Decoration plate |
| [6] | **:** | Remote controller |

**2) Fan assembly**

|  |  |  |
| --- | --- | --- |
| iNDEX | | pART NAME |
| [1] | **:** | Front fan grill |
| [2] | **:** | Grill ring |
| [3] | **:** | Blade cap |
| [4] | **:** | Fan blade |
| [5] | **:** | Grill mounting nut |
| [6] | **:** | Rear fan grill |
| [7] | **:** | Motor set |
| [8] | **:** | Metal screw |
| [9] | **:** | Metal tube |
| [10] | **:** | Fixation screw |
| [11] | **:** | Display panel |
| [12] | **:** | Control button |
| [13] | **:** | Base |
| [14] | **:** | Base nut |

How To Assemble：

1) Install fan body on the base [13] by matching the slot，and fasten the base nut [14].

2) Take out the metal tube [9] from the fan body to a corresponding length, and fasten the tube with the fixation screw [10]

3) Fasten the motor set [7] to the metal tube [9] with the specific metal screw.

4) Put the rear fan grill [6] on motor set [7]，and fasten grill mounting nut [5].

5) Install the blade [4] on motor shaft，then counterclockwisely fasten blade cap [3].

6) Plug the front fan grill [1] into the slot of the grill ring [2].

7) Put the outcome of step 6) with the rear fan grill [6] with matching the slot of the grill ring [2]..

**OPERATION**

* Please ensure the unit is in the (OFF) position before plugging into the power socket.
* Place the unit on a firm level surface.
* Avoid overloading the circuit by not plugging other high wattage products into the same power socket.
* When the unit plugs in to the power socket, the display panel will showing the corresponding room temperature.

**Display screen & Control panel**

|  |  |
| --- | --- |
| FS-40N1FY 面板(无8字摇头).JPG  1) Display panel & Control button | 2) Remote control |

**Function description**

|  |  |
| --- | --- |
| OFF: | Press this button to turn off the fan. |
| TIMER: | When the unit is in use, you can set the Timer to turn off the fan after the specified time. Press this button repeatedly to increase the Timer setting in 1 hour increments (up to a maximum of 15 hours) as indicated on the LED Display. After 5 seconds, the Timer starts. Once the Timer has run out, the unit will turn off. |
| WIND: | Press to select Normal, Natural or Sleep Mode (as indicated on the display panel).  NORMAL: Fan operates at the speed selected with “ON/SPEED or OFF” button, and remains constant during operation.  NATURAL: Natural rhythmic wind for a breeze, medium or strong air flow.. SLEEP: Operates at pre-set natural wind level (high, medium or low) for 30 min and then turns to the next lower level at the interval of 30 min, until it switches off. |
| SWING: | Press the button to select oscillation method:Simply right to left |
| ION: | Press this button to turn the Ionizer feature on/off (the fan must be operating for Ionizing to work).When the ionizer is turned on, it will assist in the purification of the room air. |
| ON/SPEED: | Press this button to start the fan at 1 Speed, in Normal Mode.  Press again to switch the fan speed from 1-2-3. |

**CLEANING AND STORAGE**

Before cleaning, turn the unit off, unplug from the power supply and wait for the unit to cool down.

To clean the unit use a soft cloth to wipe off any dust.

Please add a few drops of lubricant to the motor shaft after cleaning it to extend motor life.

**Maintainence**

Have your product repaired by a qualified person

This electric product is in accordance with the relevant safety requirements. Repairs should only be carried out by qualified persons using original spare parts, otherwise this may result in considerable danger to the user.

Please contact the store which you bought the product for after sale services if any.

**PLEASE AFFIX YOUR PROOF OF PURCHASE/RECEIPT HERE**

**IN THE EVENT OF A CLAIM UNDER WARRANTY THIS RECEIPT MUST BE PRODUCED.**

### W A R R A N T Y

1. Home of Living Brands (Pty) Limited warrants to the original purchaser of this product (“the customer”) that this product will be free of defects in quality and workmanship which under normal personal, family or household use and purpose may manifest within a period of 1 (one) year from the date of purchase (“warranty period”).
2. Where the customer has purchased a product and it breaks, is defective or does not work properly for the intended purpose, the customer must notify the supplier from whom the customer bought the product (“the supplier”) thereof within the warranty period. Any claim in terms of this warranty must be supported by a proof of purchase. If proof of purchase is not available, then repair, and/or service charges may be payable by the customer to the supplier.
3. The faulty product must be taken to the supplier's service centre to exercise the warranty.
4. The supplier will refund, repair or exchange the product in terms of this warranty subject to legislative requirements. This warranty shall be valid only where the customer has not broken the product himself, or used the product for something that it is not supposed to be used for. The warranty does not include and will not be construed to cover products damaged as a result of disaster, misuse, tamper, abuse or any unauthorised modification or repair of the product.
5. This warranty will extend only to the product provided at the date of the purchase and not to any expendables attached or installed by the customer.
6. If the customer requests that the supplier repairs the product and the product breaks or fails to work properly within 3 (three) months of the repair and not as a result of misuse, tampering or modification by or on behalf of the customer, then the supplier may replace the product or pay a refund to the customer.
7. The customer may be responsible for certain costs where products returned are not in the original packaging, or if the packaging is damaged. This will be deducted from any refund paid to the customer.

**HOME OF LIVING BRANDS (PTY) LTD (JOHANNESBURG)**

JOHANNESBURG TEL NO. (011) 490-9000

CAPE TOWN TEL NO. (021) 552-5161

DURBAN TEL NO. (031) 792-6000

www.homeoflivingbrands.co.za

www.russellhobbs.co.za